====================================
palmOne DTS Team
http://pluggedin.palmone.com
====================================

***This information is subject to the palmOne Prototype
   License/Confidentiality Agreement.


To simulate the 5-way keys, you need to use your
Desktop numeric keypad with numlock *OFF*
the arrows correspond to the 5-way arrow and the
"5" key corresponds to the center button
HOME can also be used as the center button.
On a laptop, you need to turn on the numlock to use the "5" key.
(See the Treo 600 Developer Guide for more information. The present Treo 650 Simulator has a similar
behavior as the Treo 600 Simulator. This might change in the future)

------------------------------------------
palmOne Treo 650 Simulator
------------------------------------------
July 23, 2004
NOTE: The Treo 650 Simulators take a while to start.

NOTE: If the Treo 650 Radio setting does not match the Treo 650 ROM, the Treo 650 Simulator will crash when
      you start it. To avoid this, make sure the radio settings are correct in the palmsim.ini file
	  (located in the same directory as the PalmSim.exe). For a CDMA device, the CDMA should be
	  equal to 1 and GSM should be equal to 0. For a GSM device, the CDMA should be equal to 0 and
	  GSM should be equal to 1.
	
NOTE: Hard reset on the simulator does not work, How do I hard reset the Simulator?
	  Please remove the C:\Palm\SimslotDriverVolume (This file acts as a NVFS volume) file and then
	  try to hard reset.
	
NOTE: The simulator is crashing, how can I prevent this?
      The simulator uses the C:\Palm\SimslotDriverVolume as the NVFS volume. This file may have
	  incorrect or incompatible data. Please remove this file and see if this fixes the crash.

May 14, 2004
	palmOne's Latest Simulators
	
April 30, 2004
	Initial release
